|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Organization** | **Reference citation** | **Model**  **(nozzle, pump)** | **link** |
| 1 | Institute for Implant Technology and Biomaterials, Rostock, Germany | Stiehm, M., Wüstenhagen, C., Siewert, S., Grabow, N. & Schmitz, K. (2017). Numerical simulation of pulsatile flow through a coronary nozzle model based on FDA’s benchmark geometry. *Current Directions in Biomedical Engineering*, *3*(2), 775-778. <https://doi.org/10.1515/cdbme-2017-0163> | Nozzle | <https://www.degruyter.com/document/doi/10.1515/cdbme-2017-0163/html> |
| 2 | Institute for Implant Technology and Biomaterials, Rostock, Germany | Stiehm, M., Brandt-Wunderlich, C., Siewert, S., Schmitz, K., Grabow, N., Goubergrits, L., Kühne, T., Poon, E., Ooi, A. & Barlis, P. (2020). Sensitivity analysis of FDA´s benchmark nozzle regarding in vitro imperfections - Do we need asymmetric CFD benchmarks?. *Current Directions in Biomedical Engineering*, *6*(3), 78-81. <https://doi.org/10.1515/cdbme-2020-3020> | Nozzle | <https://www.degruyter.com/document/doi/10.1515/cdbme-2020-3020/html> |
| 3 | University of Magdeburg, Germany | Janiga, Gábor. “Large eddy simulation of the FDA benchmark nozzle for a Reynolds number of 6500.” *Computers in biology and medicine* vol. 47 (2014): 113-9. doi:10.1016/j.compbiomed.2014.01.004 | Nozzle | <https://www.sciencedirect.com/science/article/abs/pii/S0010482514000067> |
| 4 | Livermore Software Technology Corp. | Huang, Chien-jung, Caldichoury, Inaki, Pin, Facundo Del, and Paz, Rodrigo R., “CFD Validations with FDA Benchmarks of Medical Devices Flows, *15th International LS-Dyna Users Conference*, 2018. | Nozzle and Pump | <https://www.researchgate.net/profile/Inaki-Caldichoury/publication/337448926_Validations_with_FDA_Benchmarks_of_Medical_Devices_Flows/links/5dd86dbc92851c1feda8cfab/Validations-with-FDA-Benchmarks-of-Medical-Devices-Flows.pdf> |
| 5 | Mississippi State University | Walters, D.K., Bhushan, S., Alam, M.F. *et al.* Investigation of a Dynamic Hybrid RANS/LES Modelling Methodology for Finite-Volume CFD Simulations. *Flow Turbulence Combust* **91,** 643–667 (2013). https://doi.org/10.1007/s10494-013-9481-9 | Nozzle | <https://link.springer.com/article/10.1007%2Fs10494-013-9481-9> |
| 6 | University of Twente, Netherlands | Jain, Karthik, Efficacy of the FDA Nozzle Benchmark and the Lattice Boltzmann Method for the Analysis of Biomedical Flows in Transitional Regime. *Medical & Biological Engineering & Computing*, 58 (2020): 1817-1830. https://doi.org/10.1007/s11517-020-02188-8 | Nozzle | <https://link.springer.com/content/pdf/10.1007/s11517-020-02188-8.pdf> |
| 7 | University of the Balearic Islands, Palma, Spain | Trias, Miquel, Arbona, Antonio, Massó, Joan, Miñano, Borja, Bona, Carles. FDA’s Nozzle Numerical Simulation Challenge: Non-Newtonian Fluid Effects and Blood Damage. PLoS ONE 9(3): (2014) e92638.  https://doi.org/10.1371/journal.pone.0092638 | Nozzle | <https://journals.plos.org/plosone/article?id=10.1371/journal.pone.0092638> |
| 8 | University of Montpellier, France | Zmijanovic, Vladeta, Mendez, Simon, Moureau Vincent, Nicoud, Frank. “About the Numerical Robustness of Biomedical Benchmark Cases: Interlaboratory FDA’s Idealized Medical Device.” *International Journal for Numerical Methods in Biomedical Engineering*. vol. 33,1 (2017): 10.1002/cnm.2789. doi:10.1002/cnm.2789 | Nozzle | <https://onlinelibrary.wiley.com/doi/full/10.1002/cnm.2789> |
| 9 | University of Montpellier, France | Nicoud F., Chnafa C., Siguenza J., Zmijanovic V., Mendez S. (2018) Large-Eddy Simulation of Turbulence in Cardiovascular Flows. In: Wriggers P., Lenarz T. (eds) Biomedical Technology. Lecture Notes in Applied and Computational Mechanics, vol 84. Springer, Cham. https://doi.org/10.1007/978-3-319-59548-1\_9 | Nozzle | <https://link.springer.com/chapter/10.1007/978-3-319-59548-1_9> |
| 10 | Imperial College London | Manchester, Emily L, and Xiao Yun Xu. “The effect of turbulence on transitional flow in the FDA's benchmark nozzle model using large-eddy simulation.” *International journal for numerical methods in biomedical engineering* vol. 36,10 (2020): e3389. doi:10.1002/cnm.3389 | Nozzle | <https://onlinelibrary.wiley.com/doi/full/10.1002/cnm.3389> |
| 11 | Universiti Teknologi Malaysia | Mohamad Shukri Zakaria, Siti Hajar Zainudin, Haslina Abdullah, Cheng See Yuan, Mohd Juzaila Abd Latif, and Kahar Osman. CFD Simulation of Non-Newtonian Effect on Hemodynamics Characteristics of Blood Flow through Benchmark Nozzle. *Journal of Advanced Research in Fluid Mechanics and Thermal Sciences*, *64*(1), 117–125. 2020 Retrieved from https://akademiabaru.com/submit/index.php/arfmts/article/view/2750 | Nozzle | <https://akademiabaru.com/submit/index.php/arfmts/article/view/2750> |
| 12 | Dassault Systemes | Santanu Chandra, Richard Swift, Ramji Kamakoti. “Modeling Hemodynamics with Abaqus/CFD Steady State Solver: FDA Benchmark Nozzle Model” | Nozzle | <https://www.adaptivecorp.com/wp-content/uploads/2017/10/Simulia-ebook-Medical-Devices-Life-Sciences-002-2.pdf#page=7> |
| 13 | Royal Institute of Technology, Stockholm, Sweden | Nour Sanchez Abad, Ricardo Vinuesa, Philipp Schlatter, Magnus Andersson, and Matts Karlsson. “Simulation Strategies for the Food and Drug Administration Nozzle Using Nek5000, AIP Advances, 10(2):025033, 2020. <https://doi.org/10.1063/1.5142703> | Nozzle | <https://aip.scitation.org/doi/full/10.1063/1.5142703> |
| 14 | University of Munich, Germany | Niklas Fehn, Wolfgang A. Wall, Martin Kronbichler. “Modern discontinuous Galerkin methods for the simulation of transitional and turbulent flows in biomedical engineering: A comprehensive LES study of the FDA benchmark nozzle model.” *International Journal for Numerical Methods in Biomedical Engineering.* (2019) 35(12):e3228, [**https://doi.org/10.1002/cnm.3228**](https://doi.org/10.1002/cnm.3228) | Nozzle | <https://onlinelibrary.wiley.com/doi/abs/10.1002/cnm.3228> |
| 15 | University of Ljubljana, Slovenia | Primož DREŠAR, Jožef Duhovnik, “A hybrid RANS-LES Computational Fluid Dynamics Simulation of an FDA Medical Device Benchmark.” Dynamics of Mechanical Systems, 25(4), (2019): <https://doi.org/10.5755/j01.mech.25.4.20105> | Nozzle | <https://www.mechanika.ktu.lt/index.php/Mech/article/view/20105> |
| 16 | Soochow University, China | Wu, P., Gao, Q. & Hsu, PL. On the representation of effective stress for computing hemolysis. *Biomech Model Mechanobiol* **18,** 665–679 (2019). https://doi.org/10.1007/s10237-018-01108-y | Nozzle and Pump | <https://link.springer.com/article/10.1007/s10237-018-01108-y> |
| 17 | Veryst Systems, MA, USA | Alireza Kermani, Amanda Vanegas, Andrew Spann, “Blood Damage Modeling of FDA Benchmark Nozzle” Comsol Conference, 2020 | Nozzle | <https://www.comsol.fr/paper/download/853441/A_Kermani%20Blood%20Damage%20Modeling%20of%20FDA%20Benchmark%20Nozzle-V5-short-B.pdf> |
| 18 | Universidad Politécnica de Madrid, Spain | Adrian Corrochano, Donnatell Xavier, Philipp Schlatter, Ricardo Vinuesa, and Soledad Le Clainche. “Flow Structures on a Planar Food and Drug Administration (FDA) Nozzle at Low and Intermediate Reynolds Number”, Fluids, 2021, 6(1),  [**https://doi.org/10.3390/fluids6010004**](https://doi.org/10.3390/fluids6010004) | Nozzle | <https://www.mdpi.com/2311-5521/6/1/4> |
| 19 | Universite de Strasbourg, France | Vincent Chabannes, Christophe Prud’Homme, Marcela Szopos, Ranine Tarabay. “High Order Finite Element Simulations For Fluid Dynamics Validated by Experimental Data From the FDA Benchmark Nozzle Model” arXiv, 2017 | Nozzle | <https://arxiv.org/abs/1701.02179> |
| 20 | Washington Univ. St. Louis, USA | Christopher John Nassau, “CFD Simulations of Cardiovascular Devices with Shape Optimization to Reduce Blood Damage Using Genetic Algorithm” Washington University at St. Louis Thesis 2020 | Nozzle and Pump | <https://openscholarship.wustl.edu/eng_etds/549/> |
| 21 | Purdue University | Jonathan E. DeGan, “Application of CFD for the Design and Evaluation of a Novel Viscous Impeller Heart Pump”, Purdue University Thesis, 2013, | Nozzle | <https://www.proquest.com/openview/d08cc2433a391cdee03a1a6ca5234bc5/1?cbl=18750&pq-origsite=gscholar> |
| 22 | Purdue University | Yann T. Delorme, Kameswararao Anupindi, Steven H. Frankel, “Large Eddy Simulation of FDA’s Idealized Medical Device”, Cardiovascular Engineering and Technology, Vol 4, Pg 392-407, 2013 | Nozzle | <https://link.springer.com/article/10.1007%2Fs13239-013-0161-7> |
| 23 | University of Sheffield, UK | Ferrari, S., Ambrogio, S., Narracott, A. J., Walker, A., Morris, P. D., and Fenner, J. W. (June 7, 2021). "An Encounter With Lattice Boltzmann for Biomedical Applications: Interactive Simulation to Support Clinical and Design Decisions." ASME. *ASME J of Medical Diagnostics*. August 2021; 4(3): 031002. <https://doi.org/10.1115/1.4051165> | Nozzle | <https://asmedigitalcollection.asme.org/medicaldiagnostics/article-abstract/4/3/031002/1109303/An-Encounter-With-Lattice-Boltzmann-for-Biomedical> |
| 24 | Livermore Software Technology Corporation, CA | Chien-Jung Huang, Facundo Del Pin, Inaki Caldichoury, Rodrigo R. Paz, “On the Performance and Accuracy of Enhanced Particle Finite Element Method (PFEM-2) in the Solution of Biomedical Benchmarks” 16th International LS-DYNA Users Conference, 2020 | Nozzle and Pump  (and IVC Model) | <https://www.dynalook.com/conferences/16th-international-ls-dyna-conference/biomedical-t6-1/t6-1-a-biomedical-067.pdf> |
| 25 | University of Rostock, Germany | Lucas Konnigk, Benjamin Torner, Martin Burschewski, Sven Grundmann and Frank-Hendrik Wurm. “Equivalent Scalar Stress Formulation Taking into Account Non-Resolved Turbulent Scales.” *Cardiovascular Engineering and Technology.* Vol. 12, 251-272, 2021 | Nozzle | <https://link.springer.com/article/10.1007/s13239-021-00526-x> |
| 26 | Lehigh University, PA | Mehdi Nikfar, Meghdad Razizadeh, Jiafeng Zhang, Ratul Paul, Zhongjun J. Wu, Yalin Liu, “Prediction of Mechanical Hemolysis in Medical Devices Via a Lagrangian Strain Based Multiscale Model.” Artificial Organs, 44(8): pgs E348-E368, 2020. <https://doi.org/10.1111/aor.13663> | Nozzle | <https://onlinelibrary.wiley.com/doi/abs/10.1111/aor.13663> |
| 27 | Livermore Software Technology Corporation | Facundo Del Pin, Chien-Jung Huang, Inaki Caldichoury and Rodrigo R. Paz. ” On the Performance and Accuracy of PFEM-2 in the Solutions of Biomedical Benchmarks.” *Computational Particle Mechanics*, Vol 7, Pgs 121-138, 2020, <https://doi.org/10.1007/s40571-019-00241-4> | Nozzle and Pump (and IVC Model) | [https://l](https://link.springer.com/article/10.1007/s40571-019-00241-4)ink.springer.com/article/10.1007/s40571-019-00241-4 |
| 28 | Livermore Software Technology Corporation | Inaki Calidichoury, Chien-jung Huang, Facundo Del Pin, Rodrigo Paz. ”Introduction of Sliding Capabilities in the ICFD LS-DYNA Solver”16th International LS-DYNA Users Conference, 2020 | Pump | <https://www.dynalook.com/conferences/16th-international-ls-dyna-conference/icfd-t12-2/t12-2-d-icfd-046.pdf> |
| 29 | Emory University, Georgia, USA | T. Passerini, A. Quaini, U. Villa, A. Veneziani, S. Canic. “Validation of an Open Source Framework for the Simulation of Blood Flow in Rigid and Deformable Vessels” International Journal for Numerical Methods in Biomedical Engineering. 29(11):1192-1213, 2013. <https://doi.org/10.1002/cnm.2568> | Nozzle | <https://onlinelibrary.wiley.com/doi/abs/10.1002/cnm.2568> |
| 30 | SISSA, Trieste, Italy and University of Houston, TX | Michele Girfoglio, Annalisa Quaini, Gianluigi Rozza. ”A Finite Volume Approximation of the Navier-Stokes equations with Equations with Nonlinear Filtering Stabilization” *Computers and Fluids*, Vol. 187, Pgs 27-45, 2019. <https://doi.org/10.1016/j.compfluid.2019.05.001> | Nozzle | <https://www.sciencedirect.com/science/article/abs/pii/S0045793019301422> |
| 31 | University of Oklahoma | Margaret L. Heck, Allen Yen, Trevor A. Snyder, Edgar A. O’Rear, Dimitrios V. Papavassiliou. “Flow-Field Simulations and Hemolysis Estimates for the Food and Drug Administration Critical Path Initiative Centrifugal Blood Pump” *Artificial Organs*. 41(10):E129-140, 2017. <https://doi.org/10.1111/aor.12837> | Pump | <https://onlinelibrary.wiley.com/doi/abs/10.1111/aor.12837> |
| 32 | University of Tehran, Iran | Mohamad Sadeq Karimi, Pooya Razzaghi, Mehrdad Raisee, Patrick Hendrick, and Ahmad Nourbakhsh. “Stochastic Simulation of the FDA Centrifugal Blood Pump Benchmark” *Biomechanics and Modeling in Mechanobiology*, Vol 20, Pgs 1871-1887, 2021, https://doi.org/10.1007/s10237-021-01482-0 | Pump | <https://link.springer.com/article/10.1007/s10237-021-01482-0> |
| 33 | Enmodes GmbH, Aachen, Germany | Sascha H. Gross-Hardt, Simon J. Sonntag, Fiete Boehning, Ulrich Steinseifer, Thomas Schmitz-Rode, Tim A.S. Kaufmann, “Crucial Aspects for Using Computational Fluid Dynamics as a Predictive Evaluation Tool for Blood Pumps” ASAIO, 65(8):864-873, (2019) doi: 10.1097/MAT.0000000000001023 | Pump | <https://journals.lww.com/asaiojournal/Fulltext/2019/11000/Crucial_Aspects_for_Using_Computational_Fluid.16.aspx> |
| 34 | Pointwise | John Chawner, “Turbulence Model Influence on Flow in the FDA Benchmark Blood Pump” Pointwise, 2020 | Pump | https://blog.pointwise.com/2020/08/06/turbulence-model-influence-on-flow-in-the-fda-benchmark-blood-pump/ |
| 35 | Koc University, Istanbul, Turkey | Caglar Ozturk, I. Basar Aka, Ismail Lazoglu, “Effect of Blade Curvature on the Hemolytic and Hydraulic Characteristics of a Centrifugal Blood Pump” *Artificial Organs,* 41(11):730-737, 2018 [https://doi.org/10.1177/0391398818785558](https://doi.org/10.1177%2F0391398818785558) | Pump | <https://journals.sagepub.com/doi/full/10.1177/0391398818785558> |
| 36 | Penn State University | Good, B. C., & Manning, K. B. (2020). Computational modeling of the Food and Drug Administration's benchmark centrifugal blood pump. *Artificial Organs*, *44*(7), E263–E276. <https://doi.org/10.1111/aor.13643> | Pump | <https://www.ncbi.nlm.nih.gov/pmc/articles/PMC7308203/> |
| 37 | | Penn State University | Tobin, N., & Manning, K. B. (2020). Large-Eddy Simulations of Flow in the FDA Benchmark Nozzle Geometry to Predict Hemolysis. *Cardiovascular Engineering and technology*, *11*(3), 254–267. https://doi.org/10.1007/s13239-020-00461-3 | Nozzle | <https://www.ncbi.nlm.nih.gov/pmc/articles/PMC7230024/> |
| 38 | | University of Tennessee | Good BC. The effects of non-Newtonian blood modeling and pulsatility on hemodynamics in the food and drug administration's benchmark nozzle model. *Biorheology*. 2021 Oct 26. doi: 10.3233/BIR-201019 | Nozzle | https://pubmed.ncbi.nlm.nih.gov/34924367/ |
| 39 | | Griffith University, Southport, Australia | Semenzin CS, Simpson B, Gregory SD, Tansley G. Validated Guidelines for Simulating Centrifugal Blood Pumps. *Cardiovasc Eng Technol*. 2021 Jun;12(3):273-285. doi: 10.1007/s13239-021-00531-0. Epub 2021 Mar 25. PMID: 33768446. | Pump | https://pubmed.ncbi.nlm.nih.gov/33768446/ |
| 40 | | University of Louisville (Kentucky) | Faghih MM, Islam A, Sharp MK. On the Discretization of the Power-Law Hemolysis Model. *J Biomech Eng*. 2021 Jan 1;143(1):011009. doi: 10.1115/1.4048075. PMID: 32793961. | Nozzle | https://pubmed.ncbi.nlm.nih.gov/32793961/ |
| 41 | | Simula Research Laboratory AS, Fornebu, Norway. | Bergersen AW, Mortensen M, Valen-Sendstad K. The FDA nozzle benchmark: "In theory there is no difference between theory and practice, but in practice there is". Int *J Numer Method Biomed Eng*. 2019 Jan;35(1):e3150. doi: 10.1002/cnm.3150. Epub 2018 Oct 22. PMID: 30211982. | Nozzle | https://pubmed.ncbi.nlm.nih.gov/30211982/ |
| 42 | | RWTH Aachen University, Germany | Gesenhues L, Pauli L, Behr M. Strain-based blood damage estimation for computational design of ventricular assist devices. *Int J Artif Organs.* 2016 Jun 15;39(4):166-70. doi: 10.5301/ijao.5000484. Epub 2016 Apr 13. PMID: 27079416. | Pump | https://pubmed.ncbi.nlm.nih.gov/27079416/ |
| 43 | | Soochow University, Suzhou, Jiangsu, China | Wu P, Groß-Hardt S, Boehning F, Hsu PL. An energy-dissipation-based power-law formulation for estimating hemolysis. *Biomech Model Mechanobiol.* 2020 Apr;19(2):591-602. doi: 10.1007/s10237-019-01232-3. Epub 2019 Oct 14. PMID: 31612342. | Nozzle and Pump | https://pubmed.ncbi.nlm.nih.gov/31612342/ |
| 44 | | University of Tehran, Iran | Mohammadi R, Karimi M, Raisee M, Sharbatdar M. Probabilistic CFD analysis on the flow field and performance of the FDA centrifugal blood pump. *Appl Mathemat Model,* (2022) 109:555-577. | Pump | https://www.sciencedirect.com/science/article/abs/pii/S0307904X22002244?via%3Dihub |
| 45 | | Soochow University, Suzhou, Jiangsu, China | Wu P. Recent advances in the application of computational fluid dynamics in the development of rotary blood pumps, *Medicine in Novel Technology and Devices,* Volume 16, 2022, 100177, ISSN 2590-0935,  https://doi.org/10.1016/j.medntd.2022.100177. | Pump | https://www.sciencedirect.com/science/article/pii/S2590093522000649?via%3Dihub |
| 46 | | University of Magdeburg, Germany | Huang F, Noël R, Berg P, Hosseini SA. Simulation of the FDA nozzle benchmark: A lattice Boltzmann study. *Comput Methods Programs Biomed.* 2022 Jun;221:106863. doi: 10.1016/j.cmpb.2022.106863. Epub 2022 May 10. PMID: 35617810. | Nozzle | https://pubmed.ncbi.nlm.nih.gov/35617810/ |
| 47 | | University of Toronto, Ontario, Canada | Haley AL, Valen-Sendstad K, Steinman DA. On delayed transition to turbulence in an eccentric stenosis model for clean vs. noisy high-fidelity CFD. *J Biomech*. 2021 Aug 26;125:110588. doi: 10.1016/j.jbiomech.2021.110588. Epub 2021 Jun 25. PMID: 34218038. | Nozzle | https://pubmed.ncbi.nlm.nih.gov/34218038/ |
| 48 | | Cumhuriyet University, Sivas, Turkey and University of Oklahoma, Norman, OK. | Avci M, Heck M, O'Rear EA, Papavassiliou DV. Hemolysis estimation in turbulent flow for the FDA critical path initiative centrifugal blood pump. *Biomech Model Mechanobiol.* 2021 Oct;20(5):1709-1722. doi: 10.1007/s10237-021-01471-3. Epub 2021 Jun 9. PMID: 34106362. | Pump | https://pubmed.ncbi.nlm.nih.gov/34106362/ |
| 49 | | FDA, Baxter Healthcare, DePuy, SimuTech, ANSYS | Morrison TM, Hariharan P, Funkhouser CM, Afshari P, Goodin M, Horner M. Assessing Computational Model Credibility Using a Risk-Based Framework: Application to Hemolysis in Centrifugal Blood Pumps. ASAIO J. 2019 May/Jun;65(4):349-360. doi: 10.1097/MAT.0000000000000996. Erratum in: ASAIO J. 2019 Nov/Dec;65(8):e100. PMID: 30973403; PMCID: PMC6493688. | Pump | https://pubmed.ncbi.nlm.nih.gov/30973403/ |
| 50 | | Mississippi State University and Cornell University | Greg W. Burgreen , Rodrigo Méndez Rojano , Mansur Zhussupbekov , James F. Antaki. Towards A Comprehensive CFD-based Model of Blood Damage. *ASAIO J*, June 2022, Vol. 68, Suppl. 2, Abstract P25, p.104. | Pump | https://asaio.org/Conference/multimedia/files/2022/journal.pdf |

**Researchers from 16 different countries have used the FDA benchmark model database in their publications (2013-2022) as of Nov. 2022.**